2015-12-11 RJS/MA/KV
ENCLOSURE CHANGE:
---------------------
11. mods to FLA enclosure to support mounting
10. mods to enclosure, spotweld corners to seal the corner

PCB CHANGE
----------------
1. extending the board outline on the short side to help soldering the enclosure.
(done)VS: Geometry of PCB: 118mm x 30mm (Rev D has size: 116mm x 29mm).

2. SMA flange to be soldered to the pcb, so there should be a strip of copper.
(Done) VS: J1 and J2 have new footprint of SMA connector: SMA_EdgeConnector.
 
-----------------------------------------------------------------------------------
2015-11-19 MA/KV
Altium CHANGE

3. While importing into DBA, we noticed MCE# for 10uF is missing: 002891 for C8, C12, C19, C23 caused by part not being picked 
from chime.library but instead elab library. needs to be fixed and pads to be checked.

(VS: done) C8, C12, C19, C23 - 10uF/25V. This time these parts are taken from CHIME_Altium.SchLib.

------------------------------------------------------------------------------------
2015-11-10 MA
4. BOM value/schematics for 1dB attenuation network is 82.1, the part number is 820Ohm. It has to be changed to 820 ohm.
(done) R6, R7, R8, R9 - 820R.


------------------------------------------------------------------------------------
2015-10-21 MA

5- Change C2 to 1pF (Rick to complete) emailed 002907 (CHECK), previously 2.7pf.
(VS. C2 - 1pF.
done)

6- Add silkscreen to the bottom if price is justified.
(done)

------------------------------------------------------------------------------------
2016-03-31 MA

7-. All vias need to have properties set to "force complete tenting on via top" and bottom UNCHECKED. Make sure the 
global setting for solder mask clearance is 12.

8- Add paste file to the generated files as per Enigma's request. (Done - RJS 2016May02)
9-. Readme file: Add filled and capped. (No longer required since Dorigo does not insist that
filling and capping are necessary - RJS 2016May02)

------------------------------------------------------------------------------------
2016-05-02  RJS
22. SMD PAD FOR POWER TO BE CONFIRMED with DORIGO (Done - thru hole with pre-tinned power harness to be used)

------------------------------------------------------------------------------------
OPEN ITEMS
23 finalize attenuator values.

